{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXM-M"]
[]
[]
[]
[]
["","","","","","2AMXM40M2V1B","2AMXM40M3V1B","2AMXM40M4V1B","2AMXM50M2V1B","2AMXM50M4V1B","2AMXM50M3V1B"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","30","","","34"]
["","","Нагрев","Сверхнизкий","м³/мин","32","","","34"]
["Уровень звуковой мощности","Отопление","","","дБ(A)","","","62","","62"]
["","Охлаждение","","","дБ(A)","","","60","","60"]
["Вентилятор","Расход воздуха","Охлаждение","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","1059","","","1200"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","1130","","","1200"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","550","550","550","550"]
["","","","Ширина","мм","765","765","765","765","765","765"]
["","","","Глубина","мм","285","285","285","285","285","285"]
["Масса","Блок","","","кг","36","36","36","41","41","41"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","760","500","500","890","500","500"]
["","","Нагревание","Самый низкий","об/мин","820","320","320","890","500","500"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","","46.0","-10","46.0"]
["","","","Макс.","°C сух.т.","46","","-10","46","-10"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-15","","-15","-15","-15.0"]
["","","","Макс.","°CWB","18","","18.0","18","18.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","46","46","","48","48"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","48","","","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","48","48","","50","50"]
["","","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","50","","","48"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","0.88","0.88","0.88","1.15","1.15","1.15"]
["","Заправка","","","tCO2Eq","0.6","0.59","0.6","0.8","0.78","0.78"]
["","ПГП","","","","675","675.0","675","675","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","20 (1)","20","20 (1)","20"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15.0","15","15","15","15.0"]
["","","IU - IU","Макс.","м","7.5","7.5","7.5","7.5","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","30","30","30","30","30","30"]
["Стандартные аксессуары","Installation manual","","","","Installation manual","1","1","1","1","1"]
["","Drain plug","","","","Drain plug","1","1","1","1","1"]
["","Screw bag","","","","Screw bag","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-230-240","220-230-240","220-240","220-230-240","220-230-240"]
["Примечания","","","","","","(1) - Для одного помещения","","","","(1) - Для одного помещения"]
["","","","","","","","(1) - Для одного помещения","","(1) - Для одного помещения"]
["","","","","","","","(2) - Рабочий диапазон см. в отдельных чертежах","","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","(3) - Электрические параметры см. в отдельных чертежах","","(3) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","","(4) - Содержит фторированные парниковые газы","","(4) - Содержит фторированные парниковые газы"]
["Стандартные аксессуары","Reducer assembly","","","","","","","1","1","1"]