{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":8,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2MXM-N"]
[]
[]
[]
[]
["","","","","","2MXM40N2V1B","2MXM50N2V1B","2MXM68N2V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","734"]
["","","","Ширина","мм","765","765","958"]
["","","","Глубина","мм","285","285","340"]
["Масса","Блок","","","кг","36","41","60"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","500","500","420"]
["","","Нагревание","Самый низкий","об/мин","320","500","420"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","","-10"]
["","","","Макс.","°C сух.т.","","","46"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","46","48"]
["","","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","48","50"]
["","","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","","48.0"]
["Хладагент","Тип","","","","R-32","R-32","R-32"]
["","Заправка","","","кг","0.88","1.15","2"]
["","Заправка","","","tCO2Eq","0.60","0.78","1.35"]
["","ПГП","","","","675","675","675.0"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","25"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 20 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15.0","15.0","15.0"]
["","","IU - IU","Макс.","м","7.5","7.5","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","30","30","50"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-230-240","220-230-240","220-240"]
["Примечания","","","","","(1) - Для одного помещения","(1) - Для одного помещения","(1) - Для одного помещения"]
["Стандартные аксессуары","Reducer assembly","","","","","1","1"]
["","Drain cap","","","","","","3"]