{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":68,"n_cols":7,"rows_kept":68,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","3AMXM-M"]
[]
[]
[]
[]
["","","","","","3AMXM52M3V1B","3AMXM52M2V1B"]
["Уровень звукового давления","Hагрев","","Ном.","дБ(A)","47"]
["","Охлаждение","","Ном.","дБ(A)","46"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Пакет для винтов","","","","1"]
["","Сливная пробка","","","","1"]
["","Сливная крышка (1)","","","","6"]
["","Сливная крышка (2)","","","","3"]
["","Отклеиваемая информационная табличка об F-газах","","","","1"]
["","Информация о дополнительном заправляемом хладагенте","","","","1"]
["Хладагент","Charge","","","TCO2Eq","1.2"]
["","ПГП","","","","675"]
["","Charge","","","кг","1.8"]
["","Тип","","","","R-32"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","420"]
["","","Hагрев","Самый низкий","об/мин","420"]
["Подсоединение труб","Перепад уровней","IU - IU","Макс.","м","7.5"]
["","","IU - OU","Макс.","м","15"]
["","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)"]
["","Общая длина трубопроводов","Система","Фактическая","м","50"]
["Компрессор","Type","","","","Герметичный компрессор ротационного типа"]
["Размеры","Блок","","Ширина","мм","868"]
["","","","Глубина","мм","320"]
["","","","Высота","мм","734"]
["Масса","Блок","","","кг","57"]
["Power supply","Phase","","","","1~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","220-240"]
["Примечания","","","","","(1) - Содержит фторированные парниковые газы"]
["","","","","","(2) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(3) - Электрические параметры см. в отдельных чертежах"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","","24"]
["","","Нагрев","Сверхнизкий","м³/мин","","24"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","847"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","847"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","734"]
["","","","Ширина","мм","","868"]
["","","","Глубина","мм","","320"]
["Масса","Блок","","","кг","","57"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","","420"]
["","","Нагревание","Самый низкий","об/мин","","420"]
["Компрессор","Type","","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","","-10"]
["","","","Макс.","°CDB","","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","-15"]
["","","","Макс.","°CWB","","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","","46"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","","47"]
["Хладагент","Тип","","","","","R-32"]
["","Заправка","","","кг","","1.80"]
["","Заправка","","","tCO2Eq","","1.2"]
["","ПГП","","","","","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","","25"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","","15"]
["","","IU - IU","Макс.","м","","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","","50"]
["Стандартные аксессуары","Installation manual","","","","","1"]
["","Drain plug","","","","","1"]
["","Screw bag","","","","","1"]
["Электропитание","Фаза","","","","","1~"]
["","Частота","","","Гц","","50"]
["","Напряжение","","","V","","220-240"]