{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-A9"]
[]
[]
[]
[]
["","","","","","5MXM90A2V1B9"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734"]
["","","","Ширина","мм","974"]
["","","","Глубина","мм","408"]
["Масса","Блок","","","кг","68"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10"]
["","","","Макс.","°C сух.т.","46"]
["Уровень звукового давления","Охлаждение","","Ном.","дБA","52"]
["","Hагрев","","Ном.","дБA","52"]
["Хладагент","Тип","","","","R-32"]
["","Заправка","","","кг","2.4"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","1.62"]
["","ПГП","","","","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","25 (1)"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","15"]
["","","IU - IU","Макс.","м","7.5"]
["Подсоединение труб","Общая длина трубопроводов","Система","Фактическая","м","75"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Сливная крышка","","","","3"]
["","Сливная пробка","","","","1"]
["","Узел переходника","","","","1"]
["","Пакет для винтов","","","","1"]
["Диапазон энергоэффективности","","","","","A+++ ~ D"]
["Электропитание","Фаза","","","","1~"]
["","Частота","","","Гц","50"]
["","Электропитание-=-Напряжение-=-В","","","В","220-240"]
["Примечания","","","","","(1) - Для одного помещения"]
["","","","","","(2) - Для комбинации с CVXM-A, FVXM-A — максимальная длина трубопровода 30 м."]
["","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(4) - Электрические параметры см. в отдельных чертежах"]
["","","","","","(5) - Содержит фторированные парниковые газы"]