{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ARXM-M9"]
[]
[]
[]
[]
["","","","","","ARXM25M3V1B9","ARXM35M3V1B9","ARXM50M3V1B9"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","735"]
["","","","Ширина","мм","765","765","825"]
["","","","Глубина","мм","285","285","300"]
["Масса","Блок","","","кг","32","32","47"]
["Compressor","Type","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10","-10"]
["","","","Макс.","°C сух.т.","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","10","10","10"]
["","","","Макс.","°CWB","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБA","46","49","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБA","47","49","49"]
["Хладагент","Тип","","","","R-32","R-32","R-32"]
["","Заправка","","","кг","0.76","0.76","1.40"]
["","Заправка","","","tCO2Eq","0.52","0.52","0.95"]
["","ПГП","","","","675.0","675.0","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20.0","20.0","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","20.0","20.0","20"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Содержит фторированные парниковые газы","(1) - Содержит фторированные парниковые газы","(1) - Рабочий диапазон см. в отдельных чертежах"]