{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":86,"n_cols":10,"rows_kept":86,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATX-KV"]
[]
[]
[]
[]
["","","","","","ATX20K5V1B","ATX25K2V1B","ATX25K5V1B","ATX35K5V1B","ATX35K2V1B (Archived)"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","","","","","43"]
["","","","Средн.","дБ(A)","","","","","35"]
["","","","Тихая работа","дБ(A)","","","","","26"]
["","","","Низк.","дБ(A)","","","","","29"]
["","Охлаждение","","Средн.","дБ(A)","","","","","34"]
["","","","Тихая работа","дБ(A)","","","","","20"]
["","","","Низк.","дБ(A)","","","","","27"]
["","","","Выс.","дБ(A)","","","","","43"]
["Стандартные аксессуары","Инструкции по установке","","","","","","","","1"]
["","Руководство по эксплуатации","","","","","","","","1"]
["","Пульт дистанционного управления","","","","","","","","1"]
["","Сухие батареи AA","","","","","","","","2"]
["","Держатель пульта дистанционного управления","","","","","","","","1"]
["","Монтажная пластина","","","","","","","","1"]
["","Титано-апатитовый фотокаталитический фильтр","","","","","","","","2"]
["","Крепежные винты внутреннего блока","","","","","","","","2"]
["Системы управления","Wired remote control","","","","","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","","","","","ARC480A11"]
["Подсоединения труб","Жидкость","","НД","мм","","","","","6.35"]
["","Газ","","НД","мм","","","","","9.50"]
["","Дренаж","","","","","","","","18"]
["Потребляемая мощность","Охлаждение","","Ном.","кВт","","","","","0.024"]
["","Hагрев","","Ном.","кВт","","","","","0.029"]
["Sound power level","Охлаждение","","","дБ(A)","","","","","58"]
["","Отопление","","","дБ(A)","","","","","58"]
["Размеры","Блок","","Ширина","мм","","","","","770"]
["","","","Глубина","мм","","","","","225"]
["","","","Высота","мм","","","","","286"]
["Корпус","Цвет","","","","","","","","Белый"]
["Масса","Блок","","","кг","","","","","9.0"]
["Power supply","Фаза","","","","","","","","1~"]
["","Частота","","","Гц","","","","","50"]
["","Наименование","","","","","","","","V1"]
["","Напряжение","","","V","","","","","220-240"]
["Примечания","","","","","","","","","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.018","0.02","0.02","0.024"]
["","Hагрев","","Ном.","кВт","0.022","0.023","0.023","0.029"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","286","286","286","286"]
["","","","Ширина","мм","770","770","770","770"]
["","","","Глубина","мм","225","225","225","225"]
["Масса","Блок","","","кг","8.5","8.5","8.5","9"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.9","10.4","10.4","11.8"]
["","","","Средн.","м³/мин","7.8","8","8","8.2"]
["","","","Низк.","м³/мин","5.8","6.1","6.1","6.3"]
["","","","Тихая работа","м³/мин","4.8","4.8","4.8","4.9"]
["","","Hагрев","Выс.","м³/мин","10.9","11.1","11.1","12.8"]
["","","Нагрев","Средн.","м³/мин","8.5","8.5","8.5","8.5"]
["","","Hагрев","Низк.","м³/мин","6.4","6.7","6.7","6.9"]
["","","","Тихая работа","м³/мин","5.2","5.2","5.2","5.2"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","55","55","55","58"]
["","Отопление","","","дБ(A)","55","55","55","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","39","40","40","43"]
["","","","Средн.","дБ(A)","33","33","33","34"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","25","26","26","27"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","20","20","20","20"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","39","40","40","43"]
["","Нагрев","","Средн.","дБ(A)","34","34","34","35"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","28","28","28","29"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","23","23","23","26"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","9.5"]
["","Дренаж","","","","18","18","18","18"]
["Системы управления","Infrared remote control","","","","ARC480A11","","","ARC480A11"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","","2","2"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Infrared remote control","","","","1","1","1","1"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]
["Системы управления","Инфракрасный пульт ДУ","","","","","ARC480A11","ARC480A11"]
["Стандартные аксессуары","AA dry-cell batteries","","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","2"]