{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":9,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXM-N"]
[]
[]
[]
[]
["","","","","","ATXM20N2V1B","ATXM25N2V1B","ATXM35N2V1B","ATXM50N2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.03","0.03","0.034","0.03"]
["","Hагрев","","Ном.","кВт","0.025","0.026","0.026","0.032"]
["Корпус","Цвет","","","","Белый","Белый","Белый","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","294","294","294","300"]
["","","","Ширина","мм","811","811","811","1040"]
["","","","Глубина","мм","272","272","272","295"]
["Масса","Блок","","","кг","10","10","10","14.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","11.1","11.1","12.3","16.1"]
["","","","Средн.","м³/мин","7.9","8.1","8.3","14.2"]
["","","","Низк.","м³/мин","6","6.2","6.4","11.6"]
["","","","Тихая работа","м³/мин","4.4","4.4","4.6","8.1"]
["","","Hагрев","Выс.","м³/мин","10.8","10.8","10.8","17.1"]
["","","Нагрев","Средн.","м³/мин","8.7","8.7","9","14.6"]
["","","Hагрев","Низк.","м³/мин","6.5","6.8","7.1","12.2"]
["","","","Тихая работа","м³/мин","5.3","5.3","5.3","10.7"]
["Уровень звуковой мощности","Охлаждение","","","дБA","58","58","58","58"]
["","Отопление","","","дБA","55","55","55","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","41","41","45","44"]
["","","","Средн.","дБA","33","33","33","40"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25","25","29","36"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","19","19","19","27"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","39","39","39","43"]
["","Нагрев","","Средн.","дБA","34","34","35","39"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","26","27","28","34"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","20","20","20","31"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.5","9.5","9.5","12.7"]
["","Дренаж","","","","18","18","18","18"]
["Системы управления","Infrared remote control","","","","ARC466A33","ARC466A33","ARC466A33","ARC466A33"]
["Системы управления","Проводной пульт дистанционного управления","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","2"]
["","Indoor unit fixing screws","","","","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]