{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","AVA-A"]
[]
[]
[]
[]
["","","","","AVA125AMVE"]
["Уровень звукового давления","Hагрев","Выс.","дБ(A)","51"]
["","","Ном.","дБ(A)","48"]
["","","Средн.","дБ(A)","46"]
["","Охлаждение","Средн.","дБ(A)","48"]
["","","Низк.","дБ(A)","46"]
["","","Выс.","дБ(A)","51"]
["Стандартные аксессуары","Винты","","","5"]
["","Инструкции по установке","","","1"]
["","Руководство по эксплуатации","","","1"]
["","Втулка","","","1"]
["","Хомуты","","","5"]
["","Изоляция фитинга для трубопровода для газа","","","1"]
["","Изоляция фитинга для трубопровода для жидкости","","","1"]
["","Влагостойкий материал","","","1"]
["","Проводка пульта дистанционного управления","","","1"]
["","Консоль для установки","","","1"]
["","Резиновая защитная прокладка отверстия","","","2"]
["","Крышка","","","1"]
["","Модель установки","","","1"]
["Системы управления","Wired remote control","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Холодопроизводительность","Общая производительность","Ном.","кВт","12.10"]
["Подсоединения труб","Жидкость","НД","мм","9.52"]
["","Газ","НД","мм","15.9"]
["","Дренаж","","","I.D. 20/O.D. 26"]
["Sound power level","Охлаждение","","дБ(A)","63"]
["Размеры","Блок","Ширина","мм","600"]
["","","Глубина","мм","350"]
["","","Высота","мм","1,850"]
["Корпус","Цвет","","","Яркий белый"]
["Масса","Блок","","кг","50"]
["Теплопроизводительность","Общая производительность","Ном.","кВт","13.5"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50/60"]
["","Напряжение","","V","220-240/220"]
["Примечания","","","","(1) - Электрические параметры см. в отдельных чертежах"]