{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","BRC1HHDW"]
[]
[]
[]
[]
["","","","","BRC1HHDAW"]
["Корпус","Цвет","","","Белый"]
["","Крышка кнопки","","","Нет"]
["","СИД работы","Цвет","","Синий индикатор состояния"]
["Размеры","Блок","Размеры-=-Блок-=-Высота-=-мм","мм","85"]
["","","Ширина","мм","85"]
["","","Глубина","мм","25"]
["","Упакованный блок","Высота","мм","50"]
["","","Ширина","мм","217"]
["","","Глубина","мм","161"]
["Масса","Блок","","kg","0.110"]
["","Упакованный блок","","kg","0.317"]
["Упаковка","Материал","","","Тонкий картон"]
["","Вес","","kg","0.0850"]
["ЖКИ","Тип","","","100 x 150 точек"]
["","Размеры","Высота","мм","40.7"]
["","","Ширина","мм","28.0"]
["","Подсветка","Цвет","","Белый"]
["Температура окружающей среды","Работа","Мин.","°C","-10"]
["","","Макс.","°C","52"]
["","Хранение","Мин.","°C","-20"]
["","","Макс.","°C","70"]
["","Температура окружающей среды-=-Относительная влажность <-=-%","","%","95"]
["Системы управления","Класс регулирования температуры","","","VI"]
["","Ƞs (Вклад  в сезонную эффективность отопления)","","%","4.0"]
["Соединительная проводка","Длина проводки","Макс.","м","500"]