{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":9,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXS-K"]
[]
[]
[]
[]
["","","","","","CTXS15K2V1B","CTXS15K3V1B","CTXS35K2V1B","CTXS35K3V1B"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","38","","41"]
["","","","Тихая работа","дБA","21","","21"]
["","","","Низк.","дБA","28","","30"]
["","Охлаждение","","Тихая работа","дБA","21","","21"]
["","","","Низк.","дБA","25","","28"]
["","","","Выс.","дБA","37","","42"]
["","","","Ном.","дБA","33"]
["","Охлаждение","","Ном.","дБA","31","","35"]
["Стандартные аксессуары","Инструкции по установке","","","","1","","1"]
["","Руководство по эксплуатации","","","","1","","1"]
["","Беспроводной пульт дистанционного управления","","","","1","","1"]
["","Батареи","","","","2","","2"]
["","Держатель пульта дистанционного управления","","","","1","","1"]
["","Монтажная пластина","","","","1","","1"]
["","Крепежные винты внутреннего блока","","","","2","","2"]
["","Титано-апатитовый фотокаталитический фильтр","","","","2","","2"]
["Системы управления","Infrared remote control","","","","ARC466A6","","ARC466A6"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","","6.35"]
["","Газ","","НД","мм","9.5","","9.5"]
["","Дренаж","","","","18","","18"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.040","","0.040"]
["","Hагрев","","Ном.","кВт","0.040","","0.040"]
["Уровень звуковой мощности","Охлаждение","","","дБA","55","","59"]
["","Отопление","","","дБA","56","","58"]
["Размеры","Блок","","Ширина","мм","780","","780"]
["","","","Глубина","мм","215","","215"]
["","","","Высота","мм","289","","289"]
["Корпус","Цвет","","","","Белый","","Белый"]
["Масса","Блок","","","кг","8","","8"]
["Вентилятор","Расход воздуха","Hагрев","Выс.","м³/мин","","","10.1"]
["","","","Низк.","м³/мин","","","6.3"]
["","","","Тихая работа","м³/мин","","","4.3"]
["","","Охлаждение","Низк.","м³/мин","","","5.2"]
["","","","Выс.","м³/мин","","","9.2"]
["","","","Тихая работа","м³/мин","","","3.9"]
["","","","Ном.","м³/мин","","","8.1"]
["","","Охлаждение","Ном.","м³/мин","","","7.2"]
["Power supply","Фаза","","","","1~","","1~"]
["","Частота","","","Гц","50","","50"]
["","Наименование","","","","V1","","V1"]
["","Напряжение","","","V","220-240","","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В"]
["Входная мощность","Охлаждение","","Ном.","кВт","","0.04","","0.040"]
["","Hагрев","","Ном.","кВт","","0.04","","0.040"]
["Корпус","Цвет","","","","","Белый","","Белый"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","289","","289"]
["","","","Ширина","мм","","780","","780"]
["","","","Глубина","мм","","215","","215"]
["Масса","Блок","","","кг","","8","","8.00"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","7.9","","9.2"]
["","","","Средн.","м³/мин","","6.3","","7.2"]
["","","","Низк.","м³/мин","","4.7","","5.2"]
["","","","Тихая работа","м³/мин","","3.9","","3.9"]
["","","Hагрев","Выс.","м³/мин","","9","","10.1"]
["","","Нагрев","Средн.","м³/мин","","7.5","","8.1"]
["","","Hагрев","Низк.","м³/мин","","6","","6.3"]
["","","","Тихая работа","м³/мин","","4.3","","4.3"]
["Уровень звуковой мощности","Охлаждение","","","дБA","","55","","59"]
["","Отопление","","","дБA","","56","","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","","37","","42"]
["","","","Средн.","дБA","","31","","35"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","","25","","28"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБA","","21","","21"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","","38","","41"]
["","Нагрев","","Средн.","дБA","","33","","36"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","","28","","30"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБA","","21","","21"]
["Подсоединение труб","Жидкость","","НД","мм","","6.35","","6.35"]
["","Газ","","НД","мм","","9.5","","9.50"]
["","Дренаж","","","","","18","","18"]
["Системы управления","Infrared remote control","","","","","ARC466A6","","ARC466A6"]
["Стандартные аксессуары","Installation manual","","","","","1","","1"]
["","Wireless remote control","","","","","1","","1"]
["","AAA dry-cell batteries","","","","","2","","2"]
["","Operation manual","","","","","1","","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2"]
["","Indoor unit fixing screws","","","","","2","","2"]
["","Mounting plate","","","","","1","","1"]
["","Remote control holder","","","","","1","","1"]
["Электропитание","Наименование","","","","","V1","","V1"]
["","Фаза","","","","","1~","","1~"]
["","Частота","","","Гц","","50","","50"]
["","Напряжение","","","V","","220-240","","220-240"]