{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":5,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKDICMPAF"]
[]
[]
[]
[]
["","","","","EKDICMPAF."]
["Температура наружного воздуха","Относительная влажность <","","%","90"]
["Размеры","Блок","Ширина","мм","300"]
["","","Глубина","мм","800"]
["","","Высота","мм","1,000"]
["Масса","Блок","","кг","50"]
["Максимальное количество подсоединяемых наружных блоков","","","","8"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50/60"]
["","Напряжение","","V","230 +/-10%"]