{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 3MXM68A2V1B9"]
["Холодопроизводительность","Ном.","","кВт","6.80"]
["Теплопроизводительность","Ном.","","кВт","8.60"]
["Номинальная эффективность","EER","","","2.73"]
["","COP","","","3.24"]
["","Годовое потребление энергии","","kWh","1245"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","D"]
["","","Нагрев","","C"]
["Охлаждение помещений","Класс энергоэффективности","","","A"]
["","Производительность","Pрасч.","кВт","6.80"]
["","SEER","","","5.42"]
["","Годовое потребление энергии","","кВтч/г","440"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A"]
["","Производительность","Pрасч.","кВт","3.60"]
["","SCOP/A","","","3.81"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.10"]
["","Годовое потребление энергии","","кВтч/г","1323"]