{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":5,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L3"]
[]
[]
[]
[]
["","","","","FCAG35BVEB / RXS35L3V1B"]
["Холодопроизводительность","Ном.","","кВт","3.40"]
["Теплопроизводительность","Ном.","","кВт","4.20"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","455"]
["","COP","","","3.50"]
["","EER","","","3.74"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A"]
["","","Нагрев","","B"]
["Подсоединение труб","Дренаж","НД","мм","VP25 (внешний диам.32, внутр. диам. 25)"]
["","Газ","НД","мм","9.50"]
["","Жидкость","НД","мм","6.35"]
["Примечания","","","","(1) - При нормальной работе: +22°C / +32°C"]
["","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","(4) - Электрические параметры см. в отдельных чертежах"]