{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Производительность по охлаждению","Общая производительность","","Ном.","kW","12.10","19.00","22.00"]
["Производительность по отоплению","Общая производительность","","Ном.","kW","13.50","22.4","24.0"]
["Корпус","Цвет","","","","Не окрашен","Не окрашен","Не окрашен"]
["","Материал","","","","Оцинкованная сталь","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["Размеры","Блок","","Высота","мм","300","470","470"]
["","","","Ширина","мм","1,400","1,490","1,490"]
["","","","Глубина","мм","700","1,100","1,100"]
["Масса","Блок","","","кг","45","104","115"]
["Требуемое пространство между подвесным потолком и перекрытием >","мм","","","","350"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","39.0","64.0","69.0"]
["","","","Средн.","м³/мин","","50","56"]
["","","","Низк.","м³/мин","28.0","36.0","43.0"]
["","","Hагрев","Выс.","м³/мин","39.0","64.0","69.0"]
["","","","Средн.","м³/мин","","50.0","56.0"]
["","","","Низк.","м³/мин","28.0","36.0","43.0"]
["","Внешнее статическое давление","","Выс.","Па","200","250","250"]
["","","","Ном.","Па","50","62","62"]
["Уровень звуковой мощности","Охлаждение","","","дБA","66","69.0","71.0"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","40","43.0","44.0"]
["","","","Medium","дБA","","39.0","40.0"]
["","","","Низк.","дБA","33","36.0","37.0"]
["","Hагрев","","Выс.","дБA","40","43.0","44.0"]
["","","","Средн.","дБA","","39.0","40.0"]
["","","","Низк.","дБA","33","36.0","37.0"]
["Подсоединения труб","Жидкость","","НД","мм","9.52","9.52","9.52"]
["","Газ","","НД","мм","15.90","19.1","22.2"]
["","Дренаж","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Высота подъема дренажа","мм","","","","625"]
["Декоративная панель","Model","","","","BYBS125DJW1"]
["","Цвет","","","","Белый (10Y9/0,5)"]
["","Размеры","","Высота","мм","55"]
["","","","Ширина","мм","1,500"]
["","","","Глубина","мм","500"]
["","Вес","","","кг","6.5"]
["Системы управления","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Стандартные аксессуары","Руководство по эксплуатации","","","","","1","1"]
["","Руководство по установке и эксплуатации","","","","1","1","1"]
["","Инструкции по установке","","","","","1","1"]
["","Общие меры предосторожности","","","","1","1","1"]
["","Соединительная труба для газа","","","","","1","1"]
["","Материал кабельного зажима","","","","","1","1"]
["","Шайба","","","","8","12","12"]
["","Пружинная шайба","","","","","2","2"]
["","Винт и шайба","","","","","45","45"]
["","Винт с шестигранной головкой с шайбой","","","","","49","49"]
["","Винты","","","","16","2","2"]
["","Винт с шестигранной головкой","","","","","2","2"]
["","Простая шайба","","","","","8","8"]
["Power supply","Наименование","","","","","VE","VE"]
["","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50/60","50/60","50/60"]
["","Напряжение","","","V","220-240/220","220-240/220","220-240/220"]
["Стандартные аксессуары","Хомут для шланга","","","","1"]
["","Сливной шланг","","","","1"]
["","Кабель общего электропитания","","","","2"]
["","Материал уплотнения (сливной шланг)","","","","1"]
["","Уплотнительный материал","","","","2"]
["","Теплоизолированная труба (жидкость)","","","","1"]
["","Теплоизолированная труба (газ)","","","","1"]
["Примечания","","","","","(1) - Электрические параметры см. в отдельных чертежах"]