{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FDXM60F3V1B9 / FDXM60F3V1B9 / RZQG125L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG125L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG125L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG100L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM35F3V1B9 / FDXM35F3V1B9 / RZQG71L8Y1B","FDXM50F3V1B9 / FDXM50F3V1B9 / RZQG71L8Y1B"]
["Холодопроизводительность","Ном.","","кВт","","","","","","","","6.80","6.80","6.80"]
["Охлаждение помещений","SEER","","","","","","","","","","4.80","4.80","4.80"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","496","496","496"]
["","Производительность","Pрасч.","кВт","","","","","","","","6.80","6.80","6.80"]
["","Класс энергоэффективности","","","","","","","","","","B","B","B"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Класс энергоэффективности","","","","","","","","","","A","A","A"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","2,211","2,211","2,211"]
["Номинальная эффективность","EER","","","","","","","","","","3.06","3.06","3.06"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Примечания","","","","","","","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м.","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м.","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","","","","","","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","","","","","(4) - Электрические параметры см. в отдельных чертежах"]