{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Уровень звукового давления","Hагрев","","Выс.","дБ(A)","35.0","35.0","","38.0"]
["","","","Средн.","дБ(A)","33.0","33.0","","35.0"]
["","","","Низк.","дБ(A)","27.0","27.0","","30.0"]
["","Охлаждение","","Средн.","дБ(A)","33.0","33.0","","35.0"]
["","","","Низк.","дБ(A)","27.0","27.0","","30.0"]
["","","","Выс.","дБ(A)","35.0","35.0","","38.0"]
["Стандартные аксессуары","Инструкции по установке","","","","1","1","","1"]
["","Руководство по эксплуатации","","","","1","1","","1"]
["","Изоляция фитинга","","","","1","1","","1"]
["","Уплотнительная подушка","","","","1","1","","1"]
["","Металлический зажим","","","","1","1","","1"]
["","Сливной шланг","","","","1","1","","1"]
["","Шайба для подвесного кронштейна","","","","8","8","","8"]
["","Уплотнительный материал","","","","2","2","","2"]
["","Зажимы","","","","6","6","","6"]
["","Крепежная пластина шайбы","","","","4","4","","4"]
["","Винты для фланцев воздуховодов","","","","1","1","","1"]
["","Воздушный фильтр","","","","1","1","","1"]
["Подсоединения труб","Жидкость","","НД","мм","6.35","6.35","","6.35"]
["","Газ","","НД","мм","9.50","9.50","","12.70"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Потребляемая мощность","Охлаждение","","Ном.","кВт","0.036","0.036","","0.060"]
["","Hагрев","","Ном.","кВт","0.036","0.036","","0.060"]
["Sound power level","Охлаждение","","","дБ(A)","53.0","53.0","","56.0"]
["","Отопление","","","дБ(A)","53.0","53.0","","56.0"]
["Размеры","Блок","","Ширина","мм","750","750","","1,150"]
["","","","Глубина","мм","620","620","","620"]
["","","","Высота","мм","200","200","","200"]
["Масса","Блок","","","кг","21","21","","28"]
["Вентилятор","Внешнее статическое давление","","Ном.","Па","30","30","","40"]
["","Расход воздуха","Hагрев","Выс.","м³/мин","8.7","8.7","","16.0"]
["","","","Средн.","м³/мин","8.0","8.0","","14.8"]
["","","","Низк.","м³/мин","7.3","7.3","","13.5"]
["","","Охлаждение","Низк.","м³/мин","7.3","7.3","","13.5"]
["","","","Средн.","м³/мин","8.0","8.0","","14.8"]
["","","","Выс.","м³/мин","8.7","8.7","","16.0"]
["Power supply","Фаза","","","","1~","1~","","1~"]
["","Частота","","","Гц","50","50","","50"]
["","Напряжение","","","V","220-240","220-240","","220-240"]
["Примечания","","","","","(1) - Электрические параметры см. в отдельных чертежах","(1) - Электрические параметры см. в отдельных чертежах","","(1) - Электрические параметры см. в отдельных чертежах"]
["Входная мощность","Охлаждение","","Ном.","кВт","","","0.060"]
["","Hагрев","","Ном.","кВт","","","0.060"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","","200"]
["","","","Ширина","мм","","","1150"]
["","","","Глубина","мм","","","620"]
["Масса","Блок","","","кг","","","28"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","","","15.8"]
["","","","Средн.","м³/мин","","","14.6"]
["","","","Низк.","м³/мин","","","13.3"]
["","","Hагрев","Выс.","м³/мин","","","15.8"]
["","","Нагрев","Средн.","м³/мин","","","14.6"]
["","","Hагрев","Низк.","м³/мин","","","13.3"]
["","Внешнее статическое давление","","Ном.","Па","","","40"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","","","55.0"]
["","Отопление","","","дБ(A)","","","55.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","","","38.0"]
["","","","Средн.","дБ(A)","","","35.0"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","","","30.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","","","38.0"]
["","Нагрев","","Средн.","дБ(A)","","","35.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","","","30.0"]
["Подсоединение труб","Жидкость","","НД","мм","","","6.35"]
["","Газ","","НД","мм","","","12.70"]
["","Дренаж","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Стандартные аксессуары","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Воздушный фильтр","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Электропитание","Фаза","","","","","","1~"]
["","Частота","","","Гц","","","50"]
["","Напряжение","","","V","","","220-240"]