{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Уровень звукового давления","Hагрев","Выс.","дБA","38"]
["","","Средн.","дБA","36"]
["","","Низк.","дБA","30"]
["","Охлаждение","Средн.","дБA","36"]
["","","Низк.","дБA","30"]
["","","Выс.","дБA","38"]
["Стандартные аксессуары","Инструкции по установке","","","1"]
["","Руководство по эксплуатации","","","1"]
["","Изоляция фитинга","","","1"]
["","Уплотнительная подушка","","","1"]
["","Металлический зажим","","","1"]
["","Сливной шланг","","","1"]
["","Шайба для подвесного кронштейна","","","8"]
["","Уплотнительный материал","","","2"]
["","Зажимы","","","6"]
["","Крепежная пластина шайбы","","","4"]
["","Винты для фланцев воздуховодов","","","1"]
["","Воздушный фильтр","","","1"]
["Подсоединения труб","Жидкость","НД","мм","6.35"]
["","Газ","НД","мм","12.7"]
["","Дренаж","","","VP20 (I.D. 20/O.D. 26)"]
["Потребляемая мощность","Охлаждение","Ном.","kW","0.060"]
["","Hагрев","Ном.","kW","0.060"]
["Уровень звуковой мощности","Охлаждение","","дБA","55"]
["","Отопление","","дБA","55"]
["Размеры","Блок","Ширина","мм","1,150"]
["","","Глубина","мм","620"]
["","","Высота","мм","200"]
["Масса","Блок","","кг","30.0"]
["Вентилятор","Внешнее статическое давление","Ном.","Па","40"]
["Power supply","Фаза","","","1~"]
["","Частота","","Гц","50/60"]
["","Наименование","","","VE"]
["","Напряжение","","V","220-240"]
["Примечания","","","","(1) - При подсоединении к наружному блоку многоблочной системы, см. технические характеристики подсоединяемого наружного блока."]