{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB9","FFA35A2VEB9","FFA50A2VEB9","FFA60A2VEB9"]
["Корпус","Материал","","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","260","260","260","260"]
["","","","Ширина","мм","575","575","575","575"]
["","","","Глубина","мм","575","575","575","575"]
["Масса","Блок","","","кг","16.0","16.0","17.5","17.5"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","9.0","10.0","12.7","14.5"]
["","","","Средн.","м³/мин","8.0","8.5","10.9","12.5"]
["","","","Низк.","м³/мин","6.5","6.5","8.6","9.5"]
["","","Hагрев","Выс.","м³/мин","9.0","10.0","12.7","14.5"]
["","","Нагрев","Средн.","м³/мин","8.0","8.5","10.9","12.5"]
["","","Hагрев","Низк.","м³/мин","6.5","6.5","8.6","9.5"]
["Уровень звуковой мощности","Охлаждение","","","дБA","48.0","51.0","56.0","60.0"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","31.0","34.0","39.0","43.0"]
["","","","Средн.","дБA","28.5","30.5","34.0","40.0"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБA","25.0","25.0","27.0","32.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","31.0","34.0","39.0","43.0"]
["","Нагрев","","Средн.","дБA","28.5","30.5","34.0","40.0"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБA","25.0","25.0","27.0","32.0"]
["Подсоединение труб","Жидкость","","НД","мм","6","6","6","6"]
["","Газ","","НД","мм","9.52","9.52","12.70","12.70"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Декоративна панель","Модель","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Цвет","","","","Белый (N9.5)","Белый (N9.5)","Белый (N9.5)","Белый (N9.5)"]
["","Размеры","","Высота","мм","46","46","46","46"]
["","","","Ширина","мм","620","620","620","620"]
["","","","Глубина","мм","620","620","620","620"]
["","Масса","","","кг","2.8","2.8","2.8","2.8"]
["Декоративная панель 2","Модель","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Цвет","","","","Серебристый","Серебристый","Серебристый","Серебристый"]
["","Размеры","","Высота","мм","46","46","46","46"]
["","","","Ширина","мм","620","620","620","620"]
["","","","Глубина","мм","620","620","620","620"]
["","Масса","","","кг","2.8","2.8","2.8","2.8"]
["Декоративная панель 3","Модель","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Цвет","","","","Белый (RAL9010)","Белый (RAL9010)","Белый (RAL9010)","Белый (RAL9010)"]
["","Размеры","","Высота","мм","55","55","55","55"]
["","","","Ширина","мм","700","700","700","700"]
["","","","Глубина","мм","700","700","700","700"]
["","Масса","","","кг","2.7","2.7","2.7","2.7"]
["Декоративная панель 4","Модель","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Цвет","","","","Белый (RAL9010)","Белый (RAL9010)","Белый (RAL9010)","Белый (RAL9010)"]
["","Размеры","","Высота","мм","55","55","55","55"]
["","","","Ширина","мм","700","700","700","700"]
["","","","Глубина","мм","700","700","700","700"]
["","Масса","","","кг","2.7","2.7","2.7","2.7"]
["Системы управления","Инфракрасный пульт ДУ","","","","BRC7EB530 (стандартная панель), BRC7F530W (белая панель), BRC7F530S (серая панель)","BRC7EB530 (стандартная панель), BRC7F530W (белая панель), BRC7F530S (серая панель)","BRC7EB530 (стандартная панель), BRC7F530W (белая панель), BRC7F530S (серая панель)","BRC7EB530 (стандартная панель), BRC7F530W (белая панель), BRC7F530S (серая панель)"]
["","Проводной пульт дистанционного управления","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Стандартные аксессуары","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Электропитание","Фаза","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240","220-240"]