{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":10,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTX-GV"]
[]
[]
[]
[]
["","","","","FTX50GV1B","FTX60GV1B","FTX71GV1B","FTX20GV1B (Archived)","FTX25GV1B (Archived)","FTX35GV1B (Archived)"]
["Уровень звукового давления","Hагрев","Выс.","дБA","42","44","46","39","40","41"]
["","","Тихая работа","дБA","30","32","34","25","25","26"]
["","","Низк.","дБA","33","35","37","28","28","29"]
["","Охлаждение","Тихая работа","дБA","31","33","34","22","22","23"]
["","","Низк.","дБA","34","36","37","25","26","27"]
["","","Выс.","дБA","43","45","46","39","40","41"]
["","","Ном.","дБA","38","40","42","34","34","35"]
["","Охлаждение","Ном.","дБA","39","41","42","33","33","34"]
["Стандартные аксессуары","Инструкции по установке","","","1","1","1","1","1","1"]
["","Руководство по эксплуатации","","","1","1","1","1","1","1"]
["","Беспроводной пульт дистанционного управления","","","1","1","1","1","1","1"]
["","Батареи","","","2","2","2","2","2","2"]
["","Держатель пульта дистанционного управления","","","1","1","1","1","1","1"]
["","Монтажная пластина","","","1","1","1","1","1","1"]
["","Крепежный винт для внутреннего блока","","","","","","2","2","2"]
["","Титано-апатитовый фотокаталитический фильтр","","","2","2","2","2","2","2"]
["Control systems","Infrared remote control","","","ARC433B70","ARC433B70","ARC433B70"]
["Подсоединение труб","Жидкость","НД","mm","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Газ","НД","mm","12.7","12.7","15.9","9.52","9.52","9.52"]
["","Дренаж","","","18","18","18","18","18","18"]
["Входная мощность","Охлаждение","Ном.","кВт","0.034","0.040 (2), 0.040 (3), 0.040 (4)","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Hагрев","Ном.","кВт","0.036","0.045 (2), 0.045 (3), 0.045 (4)","0.060 (2), 0.060 (3), 0.06 (4)"]
["Уровень звуковой мощности","Охлаждение","","дБA","59","60","63","55","56","57"]
["","Отопление","","дБA","58","59","62","55","56","57"]
["Размеры","Блок","Ширина","mm","1,050","1,050","1,050","770","770","770"]
["","","Depth","mm","238","238","238","198","198","198"]
["","","Высота","mm","290","290","290","283","283","283"]
["Корпус","Цвет","","","Белый","Белый","Белый","Белый","Белый","Белый"]
["Weight","Блок","","кг","12","12","12","7","7","7"]
["Power supply","Фаза","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","Гц","50","50","50","50","50","50"]
["","Наименование","","","V1","V1","V1","V1","V1","V1"]
["","Напряжение","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Стандартные аксессуары","Крепежные винты внутреннего блока","","","2","2"]
["Примечания","","","","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха"]
["","","","","(2) - 220 В","(2) - 220 В","(2) - 220 В"]
["","","","","(3) - 230 В","(3) - 230 В","(3) - 230 В"]
["","","","","(4) - 240В","(4) - 240В","(4) - 240В"]
["Стандартные аксессуары","Крепежные винты внутреннего блока (M4 × 12L)","","","","","2"]