{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":10,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B"]
[]
[]
[]
[]
["","","","","FTXB25B1V1","FTXB25BV1","FTXB35B1V1","FTXB35BV1","FTXB50BV1B","FTXB60BV1B"]
["Уровень звукового давления","Hагрев","Выс.","дБA","38","38","40","40","40","43"]
["","","Средн.","дБA","33","","34"]
["","","Тихая работа","дБA","25","25","23","23","32","33"]
["","","Низк.","дБA","28","28","26","26","35","37"]
["","Охлаждение","Средн.","дБA","33","","34"]
["","","Тихая работа","дБA","22","22","25","25","32","33"]
["","","Сверхвыс.","дБA","","","","","44","46"]
["","","Низк.","дБA","25","25","26","26","35","37"]
["","","Выс.","дБA","38","38","39","39","40","43"]
["","","Ном.","дБA","33","33","34","34","38","41"]
["","Охлаждение","Ном.","дБA","33","33","34","34","38","41"]
["Стандартные аксессуары","Инструкции по установке","","","1","1","1","1"]
["","Руководство по эксплуатации","","","1","1","1","1"]
["","Беспроводной пульт дистанционного управления","","","1","","1"]
["","Сухие батареи AA","","","2","","2"]
["","Держатель пульта дистанционного управления","","","1","1","1","1"]
["","Монтажная пластина","","","1","1","1","1"]
["","Крепежные винты внутреннего блока","","","2","2","2","2"]
["Системы управления","Infrared remote control","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","APGS02","APGS02"]
["Подсоединение труб","Жидкость","НД","мм","6.35","6.35","6.35","6.35"]
["","Газ","НД","мм","9.5","9.5","9.5","9.5"]
["","Дренаж","","","18","18","18","18"]
["Входная мощность","Охлаждение","Ном.","kW","0.030","0.040","0.030","0.040"]
["","Hагрев","Ном.","kW","0.040","0.040","0.040","0.040"]
["Уровень звуковой мощности","Охлаждение","","дБA","52","52","53","53","55","61"]
["","Отопление","","дБA","52","52","54","54"]
["Размеры","Блок","Ширина","мм","770","770","770","770","1,065","1,065"]
["","","Глубина","мм","216","216","216","216","224","224"]
["","","Высота","мм","283","283","283","283","310","310"]
["Корпус","Цвет","","","","","","","Белый","Белый"]
["Масса","Блок","","кг","7","8","7","8","14","14"]
["Power supply","Фаза","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","Гц","50","50","50","50","50","50"]
["","Наименование","","","V1","V1","V1","V1","V1","V1"]
["","Напряжение","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Примечания","","","","(1) - Содержит фторированные парниковые газы","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха","(1) - Содержит фторированные парниковые газы","(1) - SL: Тихий уровень работы вентилятора в установке расхода воздуха"]
["Стандартные аксессуары","Пульт дистанционного управления","","","","1","","1"]
["","Батареи","","","","2","","2"]
["","Титано-апатитовый фотокаталитический фильтр","","","","2","","2"]
["Примечания","","","","","","","","(1) - Все блоки протестированы и удовлетворяют требованиям ISO 5151 (бесканальные блоки) или ISO 13253 (канальные блоки).","(1) - Все блоки протестированы и удовлетворяют требованиям ISO 5151 (бесканальные блоки) или ISO 13253 (канальные блоки)."]
["","","","","","","","","(2) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления.","(2) - Все технические характеристики могут быть изменены изготовителем без предварительного уведомления."]