{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-A / 3MXF-A9"]
[]
[]
[]
[]
["","","","","FTXF20A5V1B / FTXF20A5V1B / FTXF20A5V1B / 3MXF52A2V1B9","FTXF20A5V1B / FTXF25A5V1B / FTXF25A5V1B / 3MXF68A2V1B9"]
["Холодопроизводительность","Мин.","","кВт","1.80","2.00"]
["","Макс.","","кВт","7.00","7.20"]
["","Ном.","","кВт","5.20","6.80"]
["Номинальная эффективность","Годовое потребление энергии","","kWh","634","977"]
["","EER","","","4.10","3.48"]
["","COP","","","3.93","3.82"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","A","A"]
["Теплопроизводительность","Ном.","","кВт","6.80","8.60"]
["","Мин.","","кВт","1.30","2.20"]
["","Макс.","","кВт","8.00","10.50"]
["Охлаждение помещений","SEER","","","","6.61"]
["","Годовое потребление энергии","","кВтч/г","","360"]
["","Производительность","Pрасч.","кВт","","6.80"]
["","Класс энергоэффективности","","","","A++"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","","5.30"]
["","SCOP/A","","","","4.03"]
["","Класс энергоэффективности","","","","A+"]
["","Годовое потребление энергии","","кВтч/г","","1,843"]