{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Уровень звукового давления","Hагрев","Выс.","дБA","39","40"]
["","","Средн.","дБA","34","34"]
["","","Тихая работа","дБA","21","21"]
["","","Низк.","дБA","28","28"]
["","Охлаждение","Medium","дБA","33","33"]
["","","Тихая работа","дБA","20","20"]
["","","Низк.","дБA","25","26"]
["","","Выс.","дБA","39","40"]
["Стандартные аксессуары","Инструкции по установке","","","1","1"]
["","Руководство по эксплуатации","","","1","1"]
["","Пульт дистанционного управления","","","1","1"]
["","Сухие батареи AAA","","","2","2"]
["","Держатель пульта дистанционного управления","","","1","1"]
["","Монтажная пластина","","","1","1"]
["","Крепежные винты внутреннего блока","","","2","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Подсоединение труб","Жидкость","НД","мм","6.35","6.35"]
["","Газ","НД","мм","9.50","9.50"]
["","Дренаж","","","18","18"]
["Входная мощность","Охлаждение","Ном.","кВт","0.017","0.019"]
["","Hагрев","Ном.","кВт","0.020","0.020"]
["Уровень звуковой мощности","Охлаждение","","дБA","55","55"]
["","Отопление","","дБA","55","55"]
["Размеры","Блок","Ширина","мм","770","770"]
["","","Глубина","мм","225","225"]
["","","Высота","мм","286","286"]
["Корпус","Цвет","","","Белый","Белый"]
["Weight","Блок","","кг","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Частота","","Гц","50","50"]
["","Напряжение","","V","220-240","220-240"]