{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":13,"n_cols":6,"rows_kept":13,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M / 5MXM-M"]
[]
[]
[]
[]
["","","","","FTXM20M2V1B / FTXM71M2V1B / 5MXM90M2V1B","FTXM42M2V1B / FTXM50M2V1B / 5MXM90M2V1B"]
["Производительность по охлаждению","Ном.","","кВт","8.00","8.00"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","996","1,006"]
["","EER","","","4.01","3.97"]
["","COP","","","3.46","3.61"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A"]
["","","Нагрев","","B","A"]
["Теплопроизводительность","Ном.","","кВт","10.00","10.00"]