{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":23,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 4MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM25R2V1B / FTXM42R2V1B / 4MXM68A2V1B9","FTXM20R5V1B / FTXM25R5V1B / FTXM25R5V1B / 4MXM68A2V1B9","FTXM20R5V1B / FTXM50R2V1B / 4MXM68A2V1B9","FTXM20R2V1B / FTXM50R2V1B / 4MXM68A2V1B9","FTXM20R5V1B / FTXM20R5V1B / FTXM25R5V1B / 4MXM68A2V1B9","FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 4MXM68A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 4MXM68A2V1B9","FTXM35R2V1B / FTXM35R2V1B / 4MXM68A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 4MXM68A2V1B9","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / 4MXM68A2V1B9","FTXM20R2V1B / FTXM20R2V1B / FTXM42R2V1B / 4MXM80A2V1B9","FTXM20R2V1B / FTXM25R2V1B / FTXM35R2V1B / 4MXM80A2V1B9","FTXM20R5V1B / FTXM20R5V1B / FTXM42R5V1B / 4MXM80A2V1B9","FTXM20R5V1B / FTXM25R5V1B / FTXM35R5V1B / 4MXM80A2V1B9","FTXM35R2V1B / FTXM42R2V1B / 4MXM80A2V1B9","FTXM35R5V1B / FTXM42R5V1B / 4MXM80A2V1B9","FTXM20R2V1B / FTXM60R2V1B / 4MXM80A2V1B9","FTXM20R5V1B / FTXM20R5V1B / FTXM20R5V1B / FTXM20R5V1B / 4MXM80A2V1B9","FTXM20R2V1B / FTXM20R2V1B / FTXM20R2V1B / FTXM20R2V1B / 4MXM80A2V1B9"]
["Холодопроизводительность","Ном.","","кВт","6.7","6.8","6.8","6.8","6.5","6.8","6.7","6.8","6.8","6.5","8.00","7.40","8.00","7.40","7.70","7.70","7.40","7.40","7.40"]
["Теплопроизводительность","Ном.","","кВт","8.30","8.60","8.60","8.60","8.20","8.60","8.30","8.60","8.60","8.20","9.40","9.30","9.40","9.30","9.00","9.00","9.30","9.60","9.60"]
["Номинальная эффективность","EER","","","3.74","3.85","3.59","3.59","4.01","3.85","3.74","3.94","3.94","4.01","3.56","3.79","3.56","3.79","3.11","3.11","3.43","4.17","4.17"]
["","COP","","","3.95","4.38","3.82","3.82","4.49","4.38","3.95","3.81","3.81","4.49","4.08","4.02","4.08","4.02","3.56","3.56","3.73","4.58","4.58"]
["","Годовое потребление энергии","","кВтч","896","883","947","947","810","883","896","863","863","810","1125","977","1125","977","1236","1236","1079","887","887"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","B","B","A","A","A"]
["","","Нагрев","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","B","B","A","A","A"]
["Охлаждение помещений","Класс энергоэффективности","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Производительность","Pрасч.","кВт","6.70","6.80","6.80","6.80","6.50","6.80","6.70","6.80","6.80","6.50","8.00","7.40","8.00","7.40","7.70","7.70","7.40","7.40","7.40"]
["","SEER","","","6.94","7.71","6.75","6.75","7.76","7.71","6.94","6.97","6.97","7.76","6.93","7.07","6.93","7.07","6.52","6.52","6.73","7.40","7.40"]
["","Годовое потребление энергии","","кВтч/г","338","309","352","352","294","309","338","342","342","294","405","370","405","370","417","417","387","351","351"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","A","A+","A","A","A+","A+","A","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Производительность","Pрасч.","кВт","4.30","5.30","4.50","4.50","5.30","5.30","4.30","4.80","4.80","5.30","5.37","5.37","5.37","5.37","4.27","4.27","4.27","6.23","6.23"]
["","SCOP/A","","","3.86","4.10","3.90","3.90","4.09","4.10","3.86","4.00","4.00","4.09","4.34","4.31","4.34","4.31","4.23","4.23","4.33","4.56","4.56"]
["","Pdh Теплопроизводительность при -10°","","кВт","3.41","4.22","3.55","3.55","4.21","4.22","3.41","3.73","3.73","4.21","4.34","4.37","4.34","4.37","3.68","3.68","3.71","4.73","4.73"]
["","Годовое потребление энергии","","кВтч/г","1559","1807","1612","1612","1814","1807","1559","1679","1679","1814","1732","1744","1732","1744","1413","1413","1382","1913","1913"]