{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":11,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS20K2V1B / RXS20L2V1B","FTXS25K2V1B / RXS25L2V1B","FTXS35K2V1B / RXS35L2V1B","FTXS42K2V1B / RXS42L2V1B","FTXS42K3V1B / RXS42L2V1B","FTXS50K2V1B / RXS50L2V1B","FTXS50K3V1B / RXS50L2V1B"]
["Холодопроизводительность","Мин.","","кВт","1.3","1.3","1.4","1.7","","1.7"]
["","Макс.","","кВт","2.8","3.2","4.0","5.0","","5.3"]
["","Ном.","","кВт","2.00","2.5","3.5","4.20","","5.00"]
["Подсоединения труб","Жидкость","НД","мм","6.35","6.35","6.35","6.35","","6.35"]
["","Газ","НД","мм","9.5","9.5","9.5","9.5","","12.7"]
["","Дренаж","OD","мм","18","18","18","18","","18"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","215","285","430","590","","705"]
["","EER","","","4.65","4.39","4.07","3.56","","3.55"]
["","COP","","","4.72","4.67","4.76","4.12","","4.00"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","A","A","A","A","","A"]
["","","Нагрев","","A","A","A","A","","A"]
["Теплопроизводительность","Ном.","","кВт","2.5","2.8","4.00","5.40","","5.80"]
["","Мин.","","кВт","1.3","1.3","1.4","1.7","","1.7"]
["","Макс.","","кВт","4.3","4.7","5.2","6.0","","6.5"]
["Примечания","","","","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС","(1) - EER/COP согласно Eurovent 2012, только для использования вне ЕС"]
["","","","","(2) - 220 В","(2) - 220 В","(2) - 220 В","(2) - 220 В","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(2) - 220 В","(2) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°"]
["","","","","(3) - 230 В","(3) - 230 В","(3) - 230 В","(3) - 230 В","(3) - 220 В","(3) - 230 В","(3) - 220 В"]
["","","","","(4) - 240В","(4) - 240В","(4) - 240В","(4) - 240В","(4) - 230 В","(4) - 240В","(4) - 230 В"]
["","","","","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - 240В","(5) - Номинальная эффективность: охлаждение при номинальной нагрузке 35°/27°, отопление при номинальной нагрузке 7°/20°","(5) - 240В"]
["Outdoor unit","","","","","","","","RXS42L","","RXS50L"]
["Холодопроизводительность","Мин.","","кВт","","","","","1.7","","1.7"]
["","Ном.","","кВт","","","","","4.20","","5.00"]
["","Макс.","","кВт","","","","","5.0","","5.3"]
["Теплопроизводительность","Мин.","","кВт","","","","","1.7","","1.7"]
["","Ном.","","кВт","","","","","5.40","","5.80"]
["","Макс.","","кВт","","","","","6.0","","6.5"]
["Номинальная эффективность","EER","","","","","","","3.35","","3.32"]
["","COP","","","","","","","4.12","","4.00"]
["","Годовое потребление энергии","","кВтч","","","","","627","","753"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","","","A","","A"]
["","","Нагрев","","","","","","A","","A"]
["Подсоединения труб","Дренаж","НД","мм","","","","","18","","18"]
["Подсоединение труб","Газ","НД","мм","","","","","12.7","","12.7"]
["","Жидкость","НД","мм","","","","","6.35","","6.35"]
["Охлаждение помещений","Класс энергоэффективности","","","","","","","A++","","A++"]
["","Производительность","Pрасч.","кВт","","","","","4.20","","5.00"]
["","SEER","","","","","","","6.80","","6.80"]
["","Годовое потребление энергии","","кВтч/г","","","","","216","","257"]
["Отопление (Умеренный климат)","Класс энергоэффективности","","","","","","","A+","","A+"]
["","Производительность","Pрасч.","кВт","","","","","4.00","","4.60"]
["","SCOP/A","","","","","","","4.20","","4.20"]
["","Годовое потребление энергии","","кВтч/г","","","","","1334","","1535"]