{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA100AVEB / RZQG100L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Холодопроизводительность","Ном.","","кВт","","","","","","","","","6.80","6.80","6.80","6.80"]
["Охлаждение помещений","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","","371","371","371","371"]
["","Производительность","Pрасч.","кВт","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Класс энергоэффективности","","","","","","","","","","","A++","A++","A++","A++"]
["Отопление (Умеренный климат)","Производительность","Pрасч.","кВт","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Класс энергоэффективности","","","","","","","","","","","A+","A+","A+","A+"]
["","Годовое потребление энергии","","кВтч/г","","","","","","","","","2,534","2,534","2,534","2,534"]
["Номинальная эффективность","Годовое потребление энергии","","кВтч","","","","","","","","","835","","","835"]
["","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["","COP","","","","","","","","","","","4.08","","","4.08"]
["","Директива о маркировке классов энергоэффективности","Охлаждение","","","","","","","","","","A","","","A"]
["","","Нагрев","","","","","","","","","","A","","","A"]
["Производительность по отоплению","Ном.","","кВт","","","","","","","","","7.50","","","7.50"]
["Примечания","","","","","","","","","","","","(1) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м.","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Номинальные значения холодопроизводительности основаны на: температура внутри помещения: 27°C с.т., 19°С вл.т., температура наружного воздуха: 35°C c.т., эквивалентная длина трубы с хладагентом: 5 м, перепад высот: 0 м."]
["","","","","","","","","","","","","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м.","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Номинальная теплопроизводительность: температура в помещении: 20°CDB, температура наружного воздуха: 7°CDB, 6°CWB, эквивалентная длина труб с хладагентом: 5 м, перепад уровня: 0 м."]
["","","","","","","","","","","","","(3) - Рабочий диапазон см. в отдельных чертежах","","","(3) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","","","","","","","","(4) - Электрические параметры см. в отдельных чертежах","","","(4) - Электрические параметры см. в отдельных чертежах"]
["Диапазон энергоэффективности","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]