{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":8,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG25K2V1B","FVXG35K2V1B","FVXG50K2V1B"]
["Входная мощность","Охлаждение","","Ном.","кВт","0.019, 0.019, 0.019","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)","0.032, 0.032, 0.032"]
["","Hагрев","","Ном.","кВт","0.022, 0.022, 0.022","0.024 (2) (1) (3), 0.024 (2) (1) (3), 0.024 (2) (1) (3)","0.035, 0.035, 0.035"]
["Корпус","Цвет","","","","Натурально белый (6.5Y 9.5/0.5)","Натурально белый (6.5Y 9.5/0.5)","Натурально белый (6.5Y 9.5/0.5)"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","600","600","600"]
["","","","Ширина","мм","950","950","950"]
["","","","Глубина","мм","215","215","215"]
["Масса","Блок","","","kg","22.0","22.0","22.0"]
["Вентилятор","Расход воздуха","Охлаждение","Выс.","м³/мин","8.9","9.1","10.6"]
["","","","Средн.","м³/мин","7.0","7.2","8.9"]
["","","","Низк.","м³/мин","5.3","5.3","7.3"]
["","","","Тихая работа","м³/мин","4.5","4.5","6.0"]
["","","Hагрев","Выс.","м³/мин","9.9","10.2","12.2"]
["","","Нагрев","Средн.","м³/мин","7.8","8.0","10.0"]
["","","Hагрев","Низк.","м³/мин","5.7","5.8","7.8"]
["","","","Тихая работа","м³/мин","4.7","5.0","6.8"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","54","55","56"]
["","Отопление","","","дБ(A)","55","56","58"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБ(A)","38","39","44"]
["","","","Средн.","дБ(A)","32","33","40"]
["","","","Уровень звукового давления-=-Охлаждение-=-Низк.-=-дБ(A)","дБ(A)","26","27","36"]
["","","","Уровень звукового давления-=-Охлаждение-=-Тихая работа-=-дБ(A)","дБ(A)","23","24","32"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБ(A)","39","40","46"]
["","Нагрев","","Средн.","дБ(A)","32","33","40"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Низк.-=-дБ(A)","дБ(A)","26","27","34"]
["","","","Уровень звукового давления-=-Hагрев-=-Тихая работа-=-дБ(A)","дБ(A)","22","23","30"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.50","9.50","12.7"]
["","Дренаж","","","","18","18","18"]
["Системы управления","Инфракрасный пульт ДУ","","","","ARC466A2","ARC466A2","ARC466A2"]
["Стандартные аксессуары","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","Installation plate","","","","1","1","1"]
["","Thermal insulation (thermal insulation tube)","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Drain hose","","","","1","1","1"]
["","Remote control holder","","","","1","1","1"]
["Электропитание","Наименование","","","","V1","V1","V1"]
["","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","В","220-240","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В"]