{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Вентилятор","Расход воздуха","Охлаждение","Сверхнизкий","м³/мин","","","30.1","30.6","48.9"]
["","","Нагрев","Сверхнизкий","м³/мин","","","25.6","27.2","43.1"]
["","","","Вентилятор-=-Расход воздуха-=-Охлаждение-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","1063","1080","1727"]
["","","Нагрев","Вентилятор-=-Расход воздуха-=-Нагрев-=-Сверхнизкий-=-фт3/мин","куб. фт/мин","","","904","960","1522"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","550","550","550","550","735"]
["","","","Ширина","мм","765","765","765","765","825"]
["","","","Глубина","мм","285","285","285","285","300"]
["Масса","Блок","","","кг","34","34","34","39","47"]
["Двигатель вентилятора","Скорость","Охлаждение","Самый низкий","об/мин","780","780","780","790","670"]
["","","Нагревание","Самый низкий","об/мин","740","740","740","780","670"]
["Compressor","Type","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-10","-10","-10","-10","-10"]
["","","","Макс.","°C сух.т.","46","46","46","46","46"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-25","-25","-25","-25","-25"]
["","","","Макс.","°CWB","18","18","18","18","18"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Выс.-=-дБ(A)","дБA","46","46","48","48","48"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Выс.-=-дБ(A)","дБA","47","47","48","48","48"]
["Хладагент","Тип","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Заправка","","","кг","1.0","1.05","1.2","1.3","1.7"]
["","Заправка","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["","ПГП","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","20","20","20","20","30"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)","0,02 (для длины труб свыше 10 м)"]
["","перепад уровня","IU - OU","Макс.","м","15","15","15","15","20"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В"]