{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B9","RXZ50NV1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","693","693","693","693","693","693"]
["","","","Ширина","мм","795","795","795","795","795","795"]
["","","","Глубина","мм","300","300","300","300","300","300"]
["Масса","Блок","","","кг","50","50","50","50","50","50"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°CDB","-10","-10","-10","-10","-10","-10"]
["","","","Макс.","°CDB","43","43","43","43","43","43"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-20","-20","-20","-20","-20","-20"]
["","","","Макс.","°CWB","18","18","18","18","18","18"]
["Уровень звукового давления","Охлаждение","","Выс.","дБA","46","46","48","48","49","49"]
["","Hагрев","","Выс.","дБA","46","46","48","48","50","50"]
["Хладагент","Тип","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Заправка","","","кг","1.34","1.34","1.34","1.34","1.34","1.34"]
["","Хладагент-=-Заправка-=-Экв. т CO2","","","Экв. т CO2","0.9","0.9","0.9","0.9","0.9","0.9"]
["","ПГП","","","","675","675","675","675","675","675"]
["Подсоединение труб","Длина трубы","Макс.","НБ - ВБ","м","10","10","10","10","10","10"]
["Подсоединения труб","перепад уровня","IU - OU","Макс.","м","8","8","8","8","8","8"]
["Стандартные аксессуары","Installation manual","","","","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~","1~","1~","1~"]
["","Частота","","","Гц","50","50","50","50","50","50"]
["","Электропитание-=-Напряжение-=-В","","","В","220-240","220-240","220-240","220-240","220-240","220-240"]
["Примечания","","","","","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В","(1) - 220 В"]
["","","","","","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В","(2) - 230 В"]
["","","","","","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В","(3) - 240В"]