{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","734","734","734"]
["","","","Ширина","мм","870","870","870"]
["","","","Глубина","мм","373","373","373"]
["Масса","Блок","","","кг","52","52","52"]
["Компрессор","Тип","","","","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа","Герметичный компрессор ротационного типа"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-20","-20","-20"]
["","","","Макс.","°C сух.т.","52","52","52"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","-21","-21","-21"]
["","","","Макс.","°CWB","18","18","18"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","62","63","64"]
["","Отопление","","","дБ(A)","62","63","64"]
["Уровень звукового давления","Охлаждение","","Уровень звукового давления-=-Охлаждение-=-Ном.-=-дБ(A)","дБ(A)","48","49","50"]
["","Hагрев","","Уровень звукового давления-=-Hагрев-=-Ном.-=-дБ(A)","дБ(A)","48","49","50"]
["Хладагент","Тип","","","","R-32","R-32","R-32"]
["","Заправка","","","кг","1.55","1.55","1.55"]
["","ПГП","","","","675","675","675"]
["","Заправка","","","tCO2Eq","1.05","1.05","1.05"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35"]
["","Газ","","НД","мм","9.52","12.7","12.7"]
["","Длина трубы","Макс.","НБ - ВБ","м","50","50","50"]
["Подсоединения труб","Дополнительная заправка хладагента","","","кг/м","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)","0,02 (для длины труб свыше 30 м)"]
["","перепад уровня","IU - OU","Макс.","м","30","30","30"]
["Стандартные аксессуары","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Электропитание","Фаза","","","","1~","1~","1~"]
["","Частота","","","Гц","50","50","50"]
["","Напряжение","","","V","220-240","220-240","220-240"]
["Примечания","","","","","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах","(1) - Рабочий диапазон см. в отдельных чертежах"]
["","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах"]
["","","","","","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы","(3) - Содержит фторированные парниковые газы"]
["Стандартные аксессуары","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]