{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Размеры","Блок","","Высота","мм","1,680"]
["","","","Ширина","мм","930"]
["","","","Глубина","мм","765"]
["Масса","Блок","","","кг","183.0"]
["Компрессор","Тип","","","","Герметичный спиральный компрессор"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","-5.0"]
["","","","Макс.","°C сух.т.","46.0"]
["","Heating","Темп. нар. возд.","Мин.","°CWB","-15.0"]
["","","","Макс.","°CWB","15.0"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","78.0"]
["","Отопление","","","дБ(A)","78.0"]
["Хладагент","Тип","","","","R-410A"]
["","Charge","","","кг","8.3"]
["","ПГП","","","","2,087.5"]
["Подсоединение труб","Жидкость","","НД","мм","9.52"]
["","Газ","","НД","мм","22.2"]
["","Длина трубы","Макс.","НБ - ВБ","м","100"]
["","","Система","Без заправки","м","30"]
["Стандартные аксессуары","Инструкции по установке","","","","1"]
["","Соединительные трубопроводы","","","","4"]
["Power supply","Фаза","","","","3N~"]
["","Частота","","","Гц","50"]
["","Напряжение","","","V","380-415"]
["Ток - 50 Гц","Макс. ток предохранителя (MFA)","","","A","25"]
["Примечания","","","","","(1) - Электропитание к внутреннему блоку FDQ выполняется отдельно"]
["","","","","","(2) - Электрические параметры см. в отдельных чертежах"]
["Размеры","Блок","","Размеры-=-Блок-=-Высота-=-мм","мм","","1680"]
["","","","Ширина","мм","","930"]
["","","","Глубина","мм","","765"]
["Масса","Блок","","","кг","","184.0"]
["Компрессор","Тип","","","","","Герметичный спиральный компрессор"]
["Рабочий диапазон","Охлаждение","Темп. нар. возд.","Мин.","°C сух.т.","","-5.0"]
["","","","Макс.","°C сух.т.","","46.0"]
["","Hагрев","Темп. нар. возд.","Мин.","°CWB","","-15.0"]
["","","","Макс.","°CWB","","15.0"]
["Уровень звуковой мощности","Охлаждение","","","дБ(A)","","78.0"]
["","Отопление","","","дБ(A)","","78.0"]
["Хладагент","Заправка","","","кг","","9.3"]
["","ПГП","","","","","2087.5"]
["","Заправка","","","tCO2Eq","","19.4"]
["Подсоединение труб","Жидкость","","НД","мм","","12.70"]
["","Газ","","НД","мм","","22.2"]
["","Длина трубы","Макс.","НБ - ВБ","м","","100"]
["","","Система","Без заправки","м","","30"]
["Стандартные аксессуары","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Электропитание","Частота","","","Гц","","50"]
["Ток — 50 Гц","Макс. ток предохранителя (MFA)","","","A","","25"]