{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Уровень звукового давления","Hагрев","","Выс.","дБA","37.0","37.0","31.0","31.0"]
["","","","Средн.","дБA","34.0","34.0","28.0","28.0"]
["","","","Низк.","дБA","29.0","29.0","25.0","25.0"]
["","Охлаждение","","Средн.","дБA","32.0","32.0","28.0","28.0"]
["","","","Низк.","дБA","29.0","29.0","25.0","25.0"]
["","","","Выс.","дБA","35.0","35.0","30.0","30.0"]
["Стандартные аксессуары","Руководство по эксплуатации","","","","1","1","1","1"]
["","Инструкции по установке","","","","1","1","1","1"]
["","Сливной шланг","","","","1","1","1","1"]
["","Металлический зажим для сливного шланга","","","","1","1","1","1"]
["","Шайба для подвесного кронштейна","","","","8","8","8","8"]
["","Винты","","","","40","40","40","40"]
["","Изоляция фитинга","","","","2","2","2","2"]
["","Уплотнительные подушки","","","","5","5","5","5"]
["","Зажимы","","","","4","4","4","4"]
["Control systems","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Подсоединение труб","Жидкость","","НД","мм","6.35","6.35","6.35","9.52"]
["","Газ","","НД","мм","9.52","12.70","12.70","15.90"]
["","Дренаж","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Уровень звуковой мощности","Охлаждение","","","дБA","60","60","56","56"]
["Размеры","Блок","","Ширина","мм","700","700","1,000","1,000"]
["","","","Глубина","мм","800","800","800","800"]
["","","","Высота","мм","245","245","245","245"]
["Корпус","Материал","","","","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали","Плита из оцинкованной стали"]
["","Colour","","","","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)","Не покрашен (оцинкован)"]
["Масса","Блок","","","кг","28.0","28.0","35.0","35.0"]
["Вентилятор","Внешнее статическое давление","","Выс.","Па","150","150","150","150"]
["","","","Ном.","Па","30","30","30","30"]
["","Расход воздуха","Hагрев","Выс.","м³/мин","15.0","15.0","18.0","18.0"]
["","","","Низк.","м³/мин","10.5","10.5","12.5","12.5"]
["","","","Средн.","м³/мин","12.5","12.5","15.0","15.0"]
["","","Охлаждение","Низк.","м³/мин","10.5","10.5","12.5","12.5"]
["","","","Средн.","м³/мин","12.5","12.5","15.0","15.0"]
["","","","Выс.","м³/мин","15.0","15.0","18.0","18.0"]
["Высота подъема дренажа","мм","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Частота","","","Гц","50/60","50/60","50/60","50/60"]
["","Напряжение","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Примечания","","","","","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука.","(1) - Уровень звуковой мощности является абсолютной величиной, указывающей мощность, производимую источником звука."]
["","","","","","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах","(2) - Электрические параметры см. в отдельных чертежах"]